Field=#~Integer~#~50|Field=Comment~String~Comment~100|Field=Description~String~Description~100|Field=Designator~String~Designator~100|Field=Footprint~String~Footprint~100|Field=LibRef~String~LibRef~100|Field=Quantity~Integer~Quantity~100|ReportField=Currency~<none>|ReportField=ProductionQuantity~1|ReportField=ProjectFileName~PI.PrjPcb|ReportField=ProjectFullPath~C:\Users\manuo\Google Drive\Teleco mío\17-18\TCI\Práctica altium\PROYECTO INTEGRADO\PI\PI.PrjPcb|ReportField=Title~Bill of Materials For Project [PI.PrjPcb] (No PCB Document Selected)|ReportField=TotalQuantity~254|ReportField=ReportTime~21:02:43|ReportField=ReportDate~01/11/2017|ReportField=ReportDateTime~01/11/2017 21:02:43|ReportField=OutputName~Bill of Materials|ReportField=OutputType~BOM_PartType|ReportField=GeneratorName~BOM|ReportField=GeneratorDescription~Bill of Materials|ReportField=VariantName~None|ReportField=Address1~|ReportField=Address2~|ReportField=Address3~|ReportField=Address4~|ReportField=Application_BuildNumber~|ReportField=ApprovedBy~|ReportField=Author~|ReportField=CheckedBy~|ReportField=CompanyName~|ReportField=CurrentDate~01/11/2017|ReportField=CurrentTime~21:02:40|ReportField=Date~|ReportField=DocumentFullPathAndName~C:\Users\manuo\Google Drive\Teleco mío\17-18\TCI\Práctica altium\PROYECTO INTEGRADO\PI\Complete circuit.SchDoc|ReportField=DocumentName~Complete circuit.SchDoc|ReportField=DocumentNumber~|ReportField=DrawnBy~|ReportField=Engineer~|ReportField=ImagePath~|ReportField=ModifiedDate~01/11/2017|ReportField=Organization~|ReportField=ProjectName~PI.PrjPcb|ReportField=Revision~|ReportField=Rule~|ReportField=SheetNumber~|ReportField=SheetTotal~|ReportField=Time~|ReportField=Title~|ReportField=DataSourceFileName~PI.PrjPcb|ReportField=DataSourceFullPath~C:\Users\manuo\Google Drive\Teleco mío\17-18\TCI\Práctica altium\PROYECTO INTEGRADO\PI\PI.PrjPcb
1|Arduino Mega 2560|||Footprint-ArduinoMega-headers|Arduino Mega 2560|1
2|Header 2|Header, 2-Pin||HDR1X2|Header 2|1
3|Cap Pol1|Polarized Capacitor (Radial)|C1, C2|RB7.6-15|Cap Pol1|2
4|CD74HC4067||CD74HC4067||CD74HC4067|8
5|LED ROJO|Typical RED, GREEN, YELLOW, AMBER GaAs LED|D1, D1, D1, D1, D1, D1, D1, D1, D2, D2, D2, D2, D2, D2, D2, D2, D3, D3, D3, D3, D3, D3, D3, D3, D4, D4, D4, D4, D4, D4, D4, D4, D5, D5, D5, D5, D5, D5, D5, D5, D6, D6, D6, D6, D6, D6, D6, D6, D7, D7, D7, D7, D7, D7, D7, D7, D8, D8, D8, D8, D8, D8, D8, D8, D9, D9, D9, D9, D9, D9, D9, D10, D10, D10, D10, D10, D10, D10, D11, D11, D11, D11, D11, D11, D11, D12, D12, D12, D12, D12, D12, D12, D13, D13, D13, D13, D13, D13, D13, D14, D14, D14, D14, D14, D14, D14, D15, D15, D15, D15, D15, D15, D15, D16, D16, D16, D16, D16, D16, D16|Diode|LED2|120
6|Res1|Resistor|R1, R1, R1, R1, R1, R1, R1, R1, R2, R2, R2, R2, R2, R2, R2, R2, R3, R3, R3, R3, R3, R3, R3, R3, R4, R4, R4, R4, R4, R4, R4, R4, R5, R5, R5, R5, R5, R5, R5, R5, R6, R6, R6, R6, R6, R6, R6, R6, R7, R7, R7, R7, R7, R7, R7, R7, R8, R8, R8, R8, R8, R8, R8, R8, R9, R9, R9, R9, R9, R9, R9, R10, R10, R10, R10, R10, R10, R10, R11, R11, R11, R11, R11, R11, R11, R12, R12, R12, R12, R12, R12, R12, R13, R13, R13, R13, R13, R13, R13, R14, R14, R14, R14, R14, R14, R14, R15, R15, R15, R15, R15, R15, R15, R16, R16, R16, R16, R16, R16, R16|AXIAL-0.3|Res1|120
7|DS1307|DC-to-DC Converter Control Circuit|U1|751-05_N|DS1307|1
8|7805||U2|7805 - duplicate|7805_1|1
