Remove Pin=U4A-9 From Net=VREF_BEACON
Remove Pin=U4A-13 From Net=XIN_BEACON
Remove Pin=U4A-14 From Net=XOUT_BEACON
Remove Pin=U4A-17 From Net=USCI_A0_STE_1
Remove Pin=U4A-18 From Net=USCI_A0_MOSI_1
Remove Pin=U4A-19 From Net=USCI_A0_MISO_1
Remove Pin=U4A-20 From Net=USCI_A0_CLK_1
Remove Pin=U4A-21 From Net=RF_SIM_UART_TX
Remove Pin=U4A-22 From Net=BUS6
Remove Pin=U4A-32 From Net=SYSTEM_ON
Remove Pin=U4A-35 From Net=EN_R_PA_BEACON
Remove Pin=U4A-42 From Net=SDN_BEACON_RADIO
Remove Pin=U4A-43 From Net=NIRQ_BEACON_RADIO
Remove Pin=U4A-44 From Net=GPIO0_BEACON_RADIO
Remove Pin=U4A-45 From Net=GPIO1_BEACON_RADIO
Remove Pin=U4A-60 From Net=USCI_A1_TX_MCU
Remove Pin=U4A-61 From Net=USCI_A1_RX_MCU
Remove Pin=U4A-69 From Net=BUS3_GPIO0
Remove Pin=U4A-70 From Net=BUS3_GPIO1
Remove Pin=U4A-71 From Net=BUS3_GPIO2
Remove Pin=U4A-72 From Net=BUS3_GPIO3
Remove Pin=U4A-73 From Net=I2C_SDA
Remove Pin=U4A-74 From Net=I2C_SCL
Remove Pin=U4A-75 From Net=ANTENNA_DEBUG
Remove Pin=U4A-84 From Net=XT2IN_BEACON
Remove Pin=U4A-85 From Net=XT2OUT_BEACON
Remove Pin=U4A-91 From Net=TCK
Remove Pin=U4A-96 From Net=TDO/TDI
