Protel Design System Design Rule Check
PCB File : C:\Users\ÓscarRamón\Desktop\TELECOMUNICACIONES\CUARTO\1º Cuatrimestre\Tecnologia de Circuitos Impresos\integrated project\proyecto altium\PROYECTO\PCB\circuito_v3.PcbDoc
Date     : 13/12/2014
Time     : 20:54:20

Processing Rule : Short-Circuit Constraint (Allowed=No) (All),(All)
Rule Violations :0

Processing Rule : Un-Routed Net Constraint ( (All) )
Rule Violations :0

Processing Rule : Clearance Constraint (Gap=10mil) (All),(All)
Rule Violations :0

Processing Rule : Power Plane Connect Rule(Relief Connect )(Expansion=20mil) (Conductor Width=10mil) (Air Gap=10mil) (Entries=4) (All)
Rule Violations :0

Processing Rule : Width Constraint (Min=10mil) (Max=10mil) (Preferred=10mil) (All)
Rule Violations :0

Processing Rule : Hole Size Constraint (Min=1mil) (Max=100mil) (All)
Rule Violations :0


Violations Detected : 0
Time Elapsed        : 00:00:00