== Land Boards I2C-TEMP-01 LED Example ==

* This example displays the temperature usiing the  [http://land-boards.com/blwiki/index.php?title=I2C-TEMP I2C-TEMP-01 card] and [https://github.com/douggilliland/lb-Arduino-Code/tree/master/libraries/LandBoards_I2CTEMP01 I2C-TEMP-01 library]
* This code uses an Arduino UNO Compatible, the [http://land-boards.com/blwiki/index.php?title=GVSDuino GVSDuino], as the processor.
* This code uses an [http://www.ebay.com/sch/i.html?_from=R40&_trksid=p2054436.m570.l1313.TR0.TRC0.H0.XMAX7219+8-Digit+red.TRS1&_nkw=MAX7219+8-Digit+red&_sacat=0 MAX7219 8-Digit 7-segment Display Module] to display the temperature.
* The [https://github.com/douggilliland/lb-Arduino-Code/tree/master/libraries/LedControl/src LedControl library is found here].

<img src="http://land-boards.com/blwiki/images/6/6b/I2C-TEMP-01-640PX.jpg" alt="I2C-TEMP-01" title="I2C-TEMP-01" />

=== Ownership ===

* Some of these files (particularly libraries) were created by others.
** There may be newer versions of these libraries "out there".
** Some libraries even have the same names but don't work the same.
* Many of these files were created by me based on the work of others.

=== Warning ===

* Use at your own risk.
** If you brick your part or it melt to a puddle, it's on you not me.
